Back to Contents Page

# Hinge Covers and Display Assembly

Dell™ Latitude™ X200 Service Manual

Hinge Covers

Display Assembly

## Hinge Covers

### Removing the Hinge Covers

1. Remove the battery.
2. On the inside of the battery bay, use your fingers to unhook the hinge covers from the back of the computer.

1 | hinge covers (2)

1. Open the display 180 degrees.
2. Push up on the hinge covers to remove them from the computer.

### Replacing the Hinge Covers

1. Open the computer all the way (180 degrees) so that it lies flat against your work surface.
2. Place the hinge covers over the display hinges:
   1. The left hinge cover fits over the power button and the right hinge cover fits over the Dell™ AccessDirect™ button. Both hinge covers pass through the display hinges to the back of the computer.
   1. Ensure that the two securing tabs on the outer edge of each hinge cover are engaged in their respective slots.
3. Press down on the top of each hinge cover to snap the hinge covers into place.
4. Close the display.
5. Press the back of each hinge cover into the back of the computer.

| NOTE: The back of each hinge cover has a tab that snaps into a slot on the back of the computer.

## Display Assembly

### Removing the Display Assembly

| NOTICE: Disconnect the computer and any attached devices from electrical outlets.

| NOTICE: To avoid ESD, ground yourself by using a wrist grounding strap or by touching an unpainted metal surface on the computer.

| NOTICE: Read "Preparing to Work Inside the Computer" before performing the following procedure.

1. Remove the battery.
2. Remove the keyboard.
3. Remove the two M2 x 6-mm screws by the display hinges on the top of the computer.

1 | M2 x 6-mm screws (2)

1. Turn the computer over, and remove the two M3 x 5-mm screws from the bottom of the computer.

1 | M3 x 5-mm screws (2)

1. Turn the computer over, and open the display 180 degrees.
2. Disconnect the antenna connector.

| NOTICE: Do not pull on the signal cable and inverter cable. Pull from the signal connector and inverter connector to disconnect the cables.

1. Disconnect the signal cable from the system board.
2. Remove the tape that secures the inverter connector, and then disconnect the inverter cable from the system board.

1 | signal cable
2 | inverter cable
3 | inverter connector
4 | signal connector

1. Move the display assembly to an upright position and pull it up out of the bottom case.

Back to Contents Page