Back to Contents Page

# Microprocessor Thermal Cooling Assembly

Dell™ Latitude™ C610/C510 Service Manual

Removing the Microprocessor Thermal Cooling Assembly

Replacing the Microprocessor Thermal Cooling Assembly

### Removing the Microprocessor Thermal Cooling Assembly

| NOTICE: Disconnect the computer and any attached devices from electrical outlets, and remove any installed batteries.

| NOTICE: To avoid ESD, ground yourself by using a wrist grounding strap or by touching an unpainted metal surface on the computer.

| NOTICE: Read "Preparing to Work Inside the Computer" before performing the following procedure.

1. Remove the hard drive.
2. Remove the keyboard.
3. Loosen the four captive screws that secure the microprocessor thermal cooling assembly to the system board.

Microprocessor Thermal Cooling Assembly Removal

1 | microprocessor thermal cooling assembly
2 | captive screws (4)
3 | right side

1. Lift the microprocessor thermal cooling assembly up and out of the system board.

### Replacing the Microprocessor Thermal Cooling Assembly

1. Place the right side of the microprocessor thermal cooling assembly under the palm rest and lower the assembly onto the system board.
2. Tighten the four captive screws, labeled 1 through 4, in consecutive order.

Back to Contents Page