Back to Contents Page

## Diskette Drive: Dell™ Latitude™ CS/CSx Portable Computers User's Guide

Your computer was shipped with a 3.5-inch diskette drive installed in the external media bay. For more information on using and installing devices in the external media bay, see "Using the External Media Bay."

The diskette drive lets you install programs and transfer data using 3.5-inch diskettes.

To use the diskette drive, insert a 3.5-inch diskette into the drive (label side up and metal end first). Push the diskette into the drive until the eject button extends outside the drive casing.

NOTICE: Do not travel with a diskette in the diskette drive. Doing so could break the eject button and damage the drive.

To remove a diskette from the drive, press the eject button to release the diskette, and then pull the diskette out of the drive.

When data is being accessed from the diskette drive, the

drive access indicator blinks.

| NOTE: As an alternative diskette drive configuration, you can connect the diskette drive to the parallel connector on the back of the computer using an optional cable available from Dell. If you are running either the Microsoft® Windows® 95 or Windows 98 operating system on your computer and the Diskette Reconfig option is enabled in the System Setup program, you do not have to reboot the computer when you connect the diskette drive to the parallel connector. If you are running the Microsoft Windows NT® operating system on your computer, reboot the computer after you connect the diskette drive.

Back to Contents Page