Back to Contents Page

# Modem

Dell™ Inspiron™ 600m Service Manual

| CAUTION: Before performing the following procedures, read the safety instructions in your Owner's Manual.

| NOTICE: To avoid electrostatic discharge, ground yourself by using a wrist grounding strap or by periodically touching an unpainted metal surface (such as the back panel) on the computer.

1. Follow the instructions in "Preparing to Work Inside the Computer."
2. Remove the keyboard.
3. Remove the display assembly.
4. Remove the palm rest.
5. Remove the M2 x 3-mm screw.

1 | modem | 4 | system board connector
2 | pull-tab | 5 | modem cable
3 | M2 x 3-mm screw |  |

1. Disconnect the modem cable from the modem.

| NOTICE: Do not disconnect the modem cable from the system board.

1. Pull up on the pull-tab to disconnect the modem from the system board connector.

| NOTICE: Ensure that the modem cable is routed correctly when you replace the modem.

1 | modem
2 | modem cable

Back to Contents Page