Back to Contents Page

# Battery Charger Board

Dell™ Latitude™ C840 Service Manual

| NOTICE: Disconnect the computer and attached devices from electrical outlets and remove any installed batteries.

| NOTICE: To avoid ESD, ground yourself by using a wrist grounding strap or by periodically touching unpainted metal on the computer.

### Removing the Battery Charger Board

1. Follow the instructions in "Preparing to Work Inside the Computer."
2. Remove the keyboard.
3. Remove the hinge cover.
4. Remove the display assembly.
5. Remove the palm rest.
6. Remove the video graphics board.
7. Lift the battery charger board out of the system board connector.

### Replacing the Battery Charger Board

Align the screw holes on the battery charger board with the screw holes on the bottom case, and then press the battery charger board down into its connector.

Back to Contents Page