Back to Contents Page

# Cooling Fan

Dell™ Latitude™ C400 Service Manual

Removing the Cooling Fan

## Removing the Cooling Fan

| NOTICE: Disconnect the computer and any attached devices from electrical outlets, and remove any installed batteries.

| NOTICE: To avoid ESD, ground yourself by using a wrist grounding strap or by touching an unpainted metal surface on the computer.

| NOTICE: Read "Preparing to Work Inside the Computer" before performing the following procedure.

1. Remove the hard drive.
2. Remove the keyboard.
3. Remove the display assembly.
4. Remove the palm rest.

Cooling Fan Removal

1 | cooling fan
2 | M2.5 x 6-mm screws (3)
3 | fan cable
4 | fan extender cable

1. Remove the fan cable from the fan extender cable that runs under the system board.
2. Remove the three M2.5 x 6-mm screws that secure the cooling fan.
3. Lift out the cooling fan.

Back to Contents Page