Back to Contents Page

# Speakers

Dell™ Latitude™ X200 Service Manual

### Removing the Speakers

| NOTICE: Disconnect the computer and any attached devices from electrical outlets.

| NOTICE: To avoid ESD, ground yourself by using a wrist grounding strap or by touching an unpainted metal surface on the computer.

| NOTICE: Read "Preparing to Work Inside the Computer" before performing the following procedure.

1. Remove the battery.
2. Remove the keyboard.
3. Remove the palm rest.
4. Remove the M2 x 4-mm screw that secures the speaker to the bottom case.

| NOTE: The left and right speakers are interchangeable.

1 | system board connector (1 per speaker)
2 | speaker connector (1 per speaker)
3 | M2 x 4-mm screw (1 per speaker)
4 | speaker cable (1 per speaker)
5 | speakers (2)

| NOTICE: Do not pull on the speaker cable. Pull from the speaker connector to disconnect the cable.

1. Disconnect the speaker cable from the system board connector.

| NOTICE: Handle the speakers with care to avoid damaging them.

1. Remove the speaker by pulling it straight up and out of the bottom case.

Back to Contents Page